

Service Bulletin for Tune Ups and Inspections

Service Agreement Benefits:

Cooling

Lifetime parts and labor warranty on most repairs

15% savings on repairs

2-tune ups per year of coverage

Replace standard 1” air filter

Flush, test and treat condensate drain line and pump

Check all motors and amp draws, will oil if applicable

Check compressor amps and windings condition

Check Freon levels and pressures

Check all start devices and wiring connections

Check temperature differential across evaporator coil

Check thermostat operation

Heating

Replace standard 1” filter

Check thermostat operation

Check flue vent pipe condition

Check draft inducer motor amps

Check flame ignition system

Check blower assembly

Check heat exchanger condition

Check electric heat strip amp draw (heat pumps)

Clean burner assembly and flame sensor

Test reversing valve operation (heat Pumps)

Test heat pump operation

Check air temperature rise

C.O.D Inspections:

Cooling

Flush and test condensate drain line and pump

Check all motors and amp draws

Check compressor amps and windings condition

Check Freon levels and pressures

Check all start devices and wiring connections

Check thermostat operation

Heating

Check thermostat operation

Check flue vent pipe condition

Check draft inducer motor amps

Check flame ignition system

Check blower assembly

Check heat exchanger condition

Check burner assembly and flame sensor condition

Check air temperature rise

Check all safeties and controls

Check heat pump operation

Check reversing valve operation (heat pumps)

Check electric heat strip amp draw (heat pumps)